!- Router RT-MI

enable

configure terminal

hostname RT-MI

end

exit

!- FastEthernet 9/0 RT-PA Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 8/0 RT-GE Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 7/0 RT-INT-MI Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- Router RT-INT-MI

enable

configure terminal

hostname RT-INT-MI

end

exit

!- FastEthernet 0/0 Sesto San Giovanni Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 1/0 Cinisello Balsamo Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

!- FastEthernet 2/0 Legnano Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

!- FastEthernet 3/0 Rho Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

!- FastEthernet 4/0 Cologno Monzese Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

!- FastEthernet 5/0 Paderno Dugano Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

!- FastEthernet 6/0 Rozzano Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

!- FastEthernet 7/0 San Giuliano Milanese Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

!- Router RT-PA

enable

configure terminal

hostname RT-PA

end

exit

!- FastEthernet 0/0 RT-MI Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 1/0 RT-FI Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 2/0 RT-RM Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 3/0 RT-TO Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 4/0 RT-INT-PA Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- Router RT-INT-PA

enable

configure terminal

hostname RT-INT-PA

end

exit

!- FastEthernet 0/0 Bagheria Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 1/0 Monreale Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 2/0 Carini Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 3/0 Partinico Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 4/0 Milsilmeri Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 5/0 Termini Imerese Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 6/0 Villabate Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 7/0 Cefalù Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- Router RT-FI

enable

configure terminal

hostname

end

exit

!- FastEthernet 0/0 RT-PA Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 1/0 RT-NA Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 2/0 RT-RM Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 3/0 RT-INT-FI Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- Router RT-INT-FI

enable

configure terminal

hostname RT-INT-FI

end

exit

!- FastEthernet 0/0 Scandicci Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 1/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 2/0 Empoli Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 3/0 Campi Bisenzio Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 4/0 Bagno a Ripoli Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 5/0 Figline e Incisa Valdarno Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 6/0 Fucecchio Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 7/0 Pontassieve Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- Router RT-TO

enable

configure terminal

hostname

end

exit

!- FastEthernet 0/0 RT-PA Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 1/0 RT-NA Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 2/0 RT-GE

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 3/0 RT-INT-TO Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- Router RT-INT-TO

enable

configure terminal

hostname

end

exit

!- FastEthernet 0/0 Moncalieri Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 1/0 Collegno Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 2/0 Rivoli Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 3/0 Nichelino Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 4/0 Settimo Torinese Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 5/0 Grugliasco Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 6/0 Chieri Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 7/0 Pinerolo Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- Router RT-NA

enable

configure terminal

hostname

end

exit

!- FastEthernet 0/0 RT-FI Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 1/0 RT-TO Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 2/0 RT-BO Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 3/0 RT-RM Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 4/0 RT-INT-NA Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- Router RT-INT-NA

enable

configure terminal

hostname

end

exit

!- FastEthernet 0/0 Giuliano in Campania Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 1/0 Torre del Greco Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 2/0 Pozzuoli Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 3/0 Casoria Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 4/0 Castellamare di Stabia Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 5/0 Afragola Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 6/0 Marano di Napoli Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 7/0 Acerra Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- Router RT-RM

enable

configure terminal

hostname

end

exit

!- FastEthernet 0/0 RT-PA Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 1/0 RT-FI Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 2/0 RT-NA Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 3/0 RT-INT-RM Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- Router RT-INT-RM

enable

configure terminal

hostname

end

exit

!- FastEthernet 0/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 1/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 2/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 3/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 4/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 5/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 6/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 7/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- Router RT-GE

enable

configure terminal

hostname

end

exit

!- FastEthernet 0/0 RT-MI Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 1/0 RT-TO Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 2/0 RT-BO Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 3/0 RT-INT-GE Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- Router RT-INT-GE

enable

configure terminal

hostname

end

exit

!- FastEthernet 0/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 1/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 2/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 3/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 4/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 5/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 6/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 7/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- Router RT-BO Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

hostname

end

exit

!- FastEthernet 0/0 RT-MI Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 1/0 RT-GE Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 2/0 RT-INT-BO Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- Router RT-INT-GE

enable

configure terminal

hostname

end

exit

!- FastEthernet 0/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 1/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 2/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 3/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 4/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 5/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 6/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit

!- FastEthernet 7/0 Net-ID <<IPv4/CIDR>> ip address <<IPv4>> <<Subnet Mask>> <<IPv4>> <<Subnet Mask>>

enable

configure terminal

interface FastEthernet

ip address <<IPv4>> <<Subnet Mask>>

no shutdown

end

exit